Panel Plunge Mountain Vista Throw

**Fabric Requirements**

1 yard Bark (Second and Fourth Border)

¼ yard Nature (Sky Top Blocks of Panel)

¼ yard Green (Ground Bottom Blocks of Panel)

1 ¼ yards Black (Window Stripes & first border)

½ yard Brown (Third Border)

1 yard Multi (4 side panel)

One panel (2/3) yard Panel-

3 ¾ yards Mountain Vista backing fabric of your choice

63" × 70" batting

Cutting:

For easier assembly, label the fabric pieces as indicated when you cut them. Note the orientation of directional prints as they will appear in the finished quilt.

*From Second and Fourth Border Fabric:*

• Cut eleven 1 ½ " × width-of-fabric (WOF) strips for the second and fourth borders.

• Cut six 2 ¼ " × WOF strips for binding.

One 5" square (**A5**) and

One 4 ½ " × 5" rectangle (**A6**).

*From Ground Block Fabric:*

• Cut one 6" × WOF strip. Sub-cut:

Two 4 ½ " × 6" rectangles (**B**),

Two 5" × 6" rectangles (**C**) and

Two 6" × 10 ½ " rectangles (**D**).

*From Black:*

• Cut six 3 ½ " × WOF strips for the first border.

• Cut ten 1 ½ " × WOF strips. Sub-cut:

Five 1 ½ " × 321/2" strips,

Five 1 ½ " × 11" strips and

Five 1 ½ " × 5" strips.

Sew the remaining strips together and cut:

Two 1 ½ " × 42 ½ " strips.

*From Third Border Fabric :*

• Cut six 2" × WOF strips for the third border.

I would stop cutting here until you come to class.

*From Side Panel Fabric Multi:*

• Cut:

Two 5" × 32 ½ " strips x length-of-fabric (LOF) strips (**E**).

• Cut:

Two 4 ½ " × 32 ½ " LOF strips (**F**),

Two 4 ½ " × 5 ½ " LOF rectangles (**G**) and

Two 5" × 5 ½ " LOF rectangles (**H**).

*From Sky Block Fabric Multi:*

• Start at the left side and work your way across the fabric width cutting the following sky units:

One 4 ½ " × 5" rectangle (**A1**),

One 5" square (**A2**),

One 5" × 10 ½ " strip (**A3**),

One 5" × 10 ½ " strip (**A4**),

*From Panel-C7464 Multi:*

• Following the quilt image for placement and orientation in the window, cut:

Two 10 ½ " × 32 ½ " strips for the middle portion of the window (**J**) Two 5 ½ " × 10 ½ " rectangles to line up below the corresponding larger panel portions (**K**).