

Instructions for Making a Mask with Elastic

|  |  |
| --- | --- |
| Cut elastic into 6 inch pieces. | |
| Insert a piece of elastic in between the two fabric pieces like this: |  |
| Stitch around all sides using a ½” seam allowance. Leave a 3” opening in one of the long sides. | (Elastic is inside the 2 layers as noted above) |
| Clip all four of the corners- Do not clip through the seams |  |
| Turn right side out – poke out the corners – press | |
| Top Stitch ¼” all the way around |  |
| Create two pleats/tucks in each side to make each side 3 ¼” in length | |
| Stitch along each side to secure pleats |  |